Master protocol

* initialize
* clear receive buffer
* send
  + write mode
  + delay
  + serial write
  + serial flush
* Read
  + read data
  + Check the check sum

Slave protocol

* Initialize
* Clear receive buffer
* Read
  + read mode
  + Check the check sum
* Send
  + Write mode
  + Delay
  + Serial write
  + Serial flush